[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: Fresno

- To: <support@gesn.com>
- Subject: Re: Fresno
- From: "Steve Knecht" <skglobal@earthlink.net>
- Date: Thu, 9 Mar 2000 20:52:24 -0800

Were these ISR type errors or hung readers? These were hung readers. If the AccuVote "stops" in the field, ask the poll worker to look through the paper slot and ask if they see a red light. If they see a red light the reader is hooped. There is always a red light at the input sensor also isn't there. I think this could be confusing?? 4. The SOS Export took 50 minutes to execute and brought the Java Script Reporting system to a halt. Also the export didn't work We'll try to get this fixed quickly. Please send us some of the larger databases including totals so we can track down the performance issues. Will do. Ken

- Prev by Date: Fw: Election problems
- Next by Date: RE: How To Duplicate VTS Install Disks
- Index(es):
  - Chronological
  - Thread