[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: Touch Screen Calibration with BS Software

- To: <rcr@dieboldes.com>
- Subject: Re: Touch Screen Calibration with BS Software
- From: "Steve Knecht" <skglobal@earthlink.net>
- Date: Wed, 24 Oct 2001 13:33:51 -0700
- References: <040401c15ca9$cb6bc2b0$3c03a8c0@obrien>

Answer: Don't put the "calibrate" button in the corner or on the edge of the touch screen where you may not be able to touch around it. Keep it in the middle somewhere and touch around it until you find it. ----- Original Message ----- From: Ian S. Piper To: rcr@dieboldes.com Sent: Wednesday, October 24, 2001 9:34 AM Subject: RE: Touch Screen Calibration with BS Software Q: How would you select an "ELO Calibration" button using the touch screen when the calibration is out to begin with? Q: Could a keyboard be used to select this function, if the touch screen is so far out of calibration that it can't be selected by using the touch screen? Ian -----Original Message----- From: owner-rcr@dieboldes.com [mailto:owner-rcr@dieboldes.com]On Behalf Of Larry Dix Sent: October 24, 2001 11:06 AM To: Rcr@Gesn. Com Subject: Touch Screen Calibration with BS Software Allow a user to do the touch screen calibration from within ballot station software. With the ultimate goal of locking users out of the OS, can a call be made to the ELO executable so that it accessed from the System Setup - Diagnostics Larry J. Dix Vice President of Operations Global Election Systems

- References:
  - RE: Touch Screen Calibration with BS Software
    - From: "Ian S. Piper" <ian@dieboldes.com>

- Prev by Date: RE: Touch Screen Calibration with BS Software
- Next by Date: RE: Touch Screen Calibration with BS Software
- Index(es):
  - Chronological
  - Thread