[Date Prev][Date Next] [Chronological] [Thread] [Top]

# reading voter card looping

- To: <bugtrack@dieboldes.com>
- Subject: reading voter card looping
- From: "Ken Clark" <ken@dieboldes.com>
- Date: Tue, 4 Jun 2002 15:33:20 -0800
- Importance: Normal

AVTS 4.3.2. If you insert a voter card partially (about in inch, say) into the reader, then the messages status message loops forever, alternating with the message “reading voter card” and “unknown card type”. The unknown card type message is inaccurate. If you insert the card upside down, you get the more accurate “card upside down” error. If a card has bad data on it (say, wrong election), then you get a wrong election error, this time in red. The card is ejected, and then the loop starts again, with the red background. Ken

- Prev by Date: RE: Lost of Stolen PCMCIA Card
- Next by Date: create voter card precinct order incorrect
- Index(es):
  - Chronological
  - Thread