[Date Prev][Date Next] [Chronological] [Thread] [Top]

# VIBS with Spyrus on non-Vibs R4

- To: "Bugtrack" <bugtrack@dieboldes.com>
- Subject: VIBS with Spyrus on non-Vibs R4
- From: "Greg Forsythe" <gfglobal@earthlink.net>
- Date: Thu, 25 Oct 2001 13:36:07 -0400

BSNT-4-1-2 non VIBS R4, GEMS-1-18-4-1, CM-0-2-10 Election mode Select asterisk on Spyrus to create VIBS card. Caution appears when voter card has been read. Touch OK and election screen with flag appears. Insert a non VIBS voter card. Instructions and following screens are magnified voter card after voter card. The only way back to a regular screen is the three fingered salute, re-boot, (I tried WD-40 and it didn't fix it). Question: Will a voter card programmed VIBS with a Spyrus inserted into a non VIBS R6 cause the same condition? If there is one VIBS out of 4 or 5 R6s in a voting location and the voter puts a VIBS card into a non VIBS R6 will that R6 have to be re-booted? Greg Forsythe Global Election Systems, Inc (416) 446-1383 office (416) 446-1425 fax (416) 464-3736 cell www.dieboldes.com

- Follow-Ups:
  - RE: VIBS with Spyrus on non-Vibs R4
    - From: "Ken Clark" <ken@dieboldes.com>

- Prev by Date: Re: BS 4.1.2 Failed to Write to Printer
- Next by Date: RE: VIBS with Spyrus on non-Vibs R4
- Index(es):
  - Chronological
  - Thread