[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: VIBS Voter Card Encoding Problem?

- To: <support@gesn.com>
- Subject: RE: VIBS Voter Card Encoding Problem?
- From: "Greg Forsythe" <gregf@gesn.com>
- Date: Thu, 13 Jun 2002 22:52:18 -0400
- Importance: Normal
- In-reply-to: <000201c2134d$b3f6ca20$2304a8c0@kclark>

According to statistics, ninety percent of visually disabled voters have some sight. In the number of demonstrations provided for the visually disabled, there has been a great deal of enthusiasm for the magnification. They get their eyes very close to the screen to see what they can. I have always wondered why we do not have the combination of the audio and magnification. My vote is for a “V”, then the “M” followed a “VM”. I do not think this would be overly complicated for the poll worker. Greg -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf Of Ken Clark Sent: Thursday, June 13, 2002 10:47 PM To: support@gesn.com Subject: RE: VIBS Voter Card Encoding Problem? It is the “expected” behavior. But presumably not the behavior you want. There are two VIBS modes, one that hides the ballot, and one that doesn’t. You control it on the Ballot Station and PCC with the “hide ballot” checkbox. The Voter Card Encoder (Spyrus) only creates the cards that don’t hide the ballot – there is no analogous checkbox to hide the ballot. It would be pretty easy to change the software to have an “H” option, in addition to “V” and “M”. H would mean a hidden VIBS ballot. I thought about it at the time V was added, but was (and am) worried that the number of flags was getting out of hand. Also, that H gives you a VIBS ballot didn’t strike me as very obvious. The other possibility is to have a setup parameter as part of the Supervisor mode which dictates whether VIBS ballots are hidden or not. After it is set up, all subsequent uses of V are either hidden or not, depending. Do you have any thoughts/suggestions on the matter? The H thing is a little easier to implement, but not by much. If we do the option thing, what should be the default? Do more people want the VIBS ballot hidden, or visible? Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf Of Mark S Earley Sent: Thursday, June 13, 2002 5:25 PM To: Support Subject: VIBS Voter Card Encoding Problem? During GA Training today, created a VIBS Voter Card by using the * method on the Encoder. Inserted into machine in Election Mode and heard audio ballot but screen was not hidden. Did not have a keyboard or headphone attached – none available. Is this the expected behavior? Did I leave out a step to make the screen go blank while voting the audio ballot? Possibly programmed Encoder improperly? Mark Earley 850 422-2100 - office/fax 850 322-3226 - cell

- Follow-Ups:
  - RE: VIBS Voter Card Encoding Problem?
    - From: "Mark S Earley" <meglobal@earthlink.net>

- References:
  - RE: VIBS Voter Card Encoding Problem?
    - From: "Ken Clark" <ken@gesn.com>

- Prev by Date: RE: Programming Encoder w/ 1 ballot style, multiple base pcts
- Next by Date: Re: VIBS Voter Card Encoding Problem?
- Index(es):
  - Chronological
  - Thread