[Date Prev][Date Next] [Chronological] [Thread] [Top]

# R6 units freezing - how many elections on a unit?

- To: "SUPPORT \(E-mail\)" <support@gesn.com>
- Subject: R6 units freezing - how many elections on a unit?
- From: "Tari Runyan" <tarir@dieboldes.com>
- Date: Thu, 9 Jan 2003 16:50:33 -0700

this is from a customer - I like the Geek squad mention - anyone got any ideas - they will send the TS units in - but the question is why and what?
thanks
Tari
During this past election we had 5 TS units
(R6), which repeatedly froze during the process of voting. All connections were checked and there wasn't any indication of power fluctuations. Each
unit was connected to an UPS (not in series). Rebooting corrected the problem, but it did reoccur frequently. Do you have any advice? Is this an hardware problem or a software problem?
I was also trying to get a feel for how many elections we should leave in
the backup directories on the TS. I know that it depends on the election
and the number of times the unit was used. Does the Geek Squad have any
recommendations?

- Follow-Ups:
  - Re: R6 units freezing - how many elections on a unit?
    - From: "Talbot Iredale" <tiredale@dieboldes.com>
  - RE: R6 units freezing - how many elections on a unit?
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Fw: Bug#615
- Next by Date: RE: R6 units freezing - how many elections on a unit?
- Index(es):
  - Chronological
  - Thread