[Date Prev][Date Next] [Chronological] [Thread] [Top]

# System Setup Diagnostic saved settings

- To: "Bugtrack@Gesn. Com" <bugtrack@dieboldes.com>
- Subject: System Setup Diagnostic saved settings
- From: "Larry Dix" <ljdglobal@dieboldes.com>
- Date: Thu, 25 Oct 2001 16:58:46 -0500
- Importance: Normal

Posted on behalf of Diebold while doing system setup. After running a smart card reader diagnostic, and removing the tested smart card when it is ejected, the program will leave the system setup routine and dump you back to the initial menu screen. Any settings that may have been adjusted in the setup are not saved to internal flash filesystem because you aren't given the opportunity to press OK at the bottom of the system setup page. The changed settings are still in DRAM but when the unit is powered off, they're lost. Larry J. Dix Vice President of Operations Global Election Systems

- Prev by Date: RE: BSCE-4.1.2: Can't select Language via VIBS.
- Next by Date: RE: BSCE-4.1.2: Can't select Language via VIBS.
- Index(es):
  - Chronological
  - Thread