[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AV-OS LCD Displays

- To: <support@gesn.com>
- Subject: RE: AV-OS LCD Displays
- From: "Ian S. Piper" <ian@gesn.com>
- Date: Fri, 18 Jan 2002 10:31:37 -0600
- Importance: Normal
- In-reply-to: <01c201c1a036$343a5200$b3d6fc9e@default>

I haven't heard of any problems experienced with the LCD displays on the production floor. I know that cold temperatures can cause the displays to be dim. We adjust the contrast trimmer during the manufacturing. But if there is a manufacturing process problem, you can check the adjustment on the trim pot. It's on the CPU board, labeled as RV1, and it's located on the front edge of the CPU board, just to the right of the LCD/Printer bracket. You'd need a small flat blade screwdriver to adjust the trim pot. If there is a malfunction with the LCD display, it can be replaced in the field. You'd need a small Philips (#1) screwdriver to remove the four screws that secure the LCD to the bracket. Sincerely, Ian S. Piper Manufacturing Director Global Election Systems, Inc. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Steve Knecht Sent: January 18, 2002 9:39 AM To: Global Support Subject: AV-OS LCD Displays I have several units delivered to Placer where half the LCD character is dimmed making it hard to read. Any experience with that in McKinney? Can LCD's be replaced in the field or does it require return to McKinney? Steve Knecht Diebold Election Systems 415-893-9941 office 415-893-9951 fax 415-225-6591 cell

- References:
  - AV-OS LCD Displays
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Re: AV-OS LCD Displays
- Next by Date: RE: VIBS Keypad
- Index(es):
  - Chronological
  - Thread