[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Fw: Modem Lights

- To: "Global Support" <support@gesn.com>
- Subject: Fw: Modem Lights
- From: "Steve Knecht" <skglobal@earthlink.net>
- Date: Mon, 1 Nov 1999 09:01:47 -0800

I believe i received email from Mike indicating 3 and 8 down. Is Charlie's note relevant and maybe the cause of my errant lights? -----Original Message----- From: Charlies Mail <ccglobal@earthlink.net> To: Steve Knecht <skglobal@earthlink.net> Date: Monday, November 01, 1999 8:53 AM Subject: Re: Modem Lights My notes say that, for incoming, dipswitches 4 & 8 should be down..... (my notes are as old as I am) Charlie -----Original Message----- From: Steve Knecht <skglobal@earthlink.net> To: Global Support <support@gesn.com> Date: Monday, November 01, 1999 10:39 morning Subject: Modem Lights I don't know whether this is a problem or not. Does anyone else. The normal lights on the US Robotics Modem light up when the Com port is started (AA = Auto Answer, TR = Terminal Ready, and CS=Clear to Send). However, when the 1st poll site uses modem, it does not recycle back to this state, but also has the ARQ/FAX light, which stays lit. Is this a problem?? According to Manual light indicates ARQ/ Error Control / FAX Fax Operations Data Mode: Automatic Repeat Request. ON if modem is set to &M4 or &M5 and successfully establishes an error control connection. Flashes when modem retransmits data to remote modem. Fax Mode: Flashes to indicate fax mode. The light is just constantly on after 1st transmission. I have 3 and 8 in "down" position. Comments?

- Follow-Ups:
  - RE: Modem Lights
    - From: "Ken Clark" <ken@gesn.com>

- Prev by Date: Modem Lights
- Next by Date: RE: Modem Lights
- Index(es):
  - Chronological
  - Thread