[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Environmental Specs for the AV-TS R6 Unit

- To: "Steve Moreland \(E-mail\)" <stevem@gesn.com>
- Subject: Environmental Specs for the AV-TS R6 Unit
- From: "Ian S. Piper" <ian@gesn.com>
- Date: Wed, 13 Feb 2002 15:58:11 -0600
- Cc: "Global Support \(E-mail\)" <support@gesn.com>
- Importance: Normal

Steve:
The environmental specs for the R6 unit are incorrectly noted in the User's Guide. The specs should read:
The operating temperature range is +5C to +40C ( +41F to +104F. ) Relative Humidity is 10% to 90% (non-condensing.)
The storage temperature range is -15C to +55C ( +5F to +131F. ) Relative Humidity is 10% to 90% (non-condensing).
Sincerely,
Ian S. Piper
Diebold Election Systems, Inc.

- Prev by Date: RE: Sound Card for VIBS
- Next by Date: Re: Sound Card for VIBS
- Index(es):
  - Chronological
  - Thread