[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: WinCE212-011120

- To: <support@gesn.com>
- Subject: RE: WinCE212-011120
- From: "Ian S. Piper" <ian@gesn.com>
- Date: Tue, 20 Nov 2001 12:58:51 -0600
- Importance: Normal
- In-reply-to: <015701c171f4$96a0e410$0a04a8c0@gesn.com>

Slot 0 (lower slot) is the only place that bootloader program looks at when determining if there is an installation file available on the flash card. Ian -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Nel Finberg Sent: November 20, 2001 12:53 PM To: support@gesn.com Subject: Re: WinCE212-011120 Why does the card have to be installed in the lower slot? Nel ----- Original Message ----- From: Talbot Iredale To: Software Announcements Sent: Tuesday, November 20, 2001 9:55 AM Subject: WinCE212-011120 The WCE212-011120 image is now on the ftp site in the BS4Fix directory. The password is handj91ndj09s To load this image unzip it to a PCMCIA storage card and insert the storage card in the AVTS-R6 units lower PCMCIA slot and then turn the system on. The boot loader will detect the new image and load it into the Flash. This fixes the 'clicking' problem with the sound, therefore unless you are having a real problem with the 'clicking' do not bother to load this release. Tab

- References:
  - Re: WinCE212-011120
    - From: "Nel Finberg" <nel@gesn.com>

- Prev by Date: Re: ABO file used in Florida
- Next by Date: CA. March Primary
- Index(es):
  - Chronological
  - Thread