[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Numeric Key row inoperable using BS 4.1.1.1

- To: "bugtrack" <bugtrack@dieboldes.com>
- Subject: RE: Numeric Key row inoperable using BS 4.1.1.1
- From: "Jeff Hallmark" <jeffh@dieboldes.com>
- Date: Wed, 24 Oct 2001 17:07:36 -0500
- Importance: Normal

Ken, This is not fixed... totally. For a multiple language election the Select Language feature in VIBS uses t he keypad numbers starting with "1". Testing a two language selection using the "1" and "2" keys doesn't work. jwh I think this is "fixed" in 4.1.2. It is mostly academic however. You can't run an election with the security door unlocked. If you want to meet TX fist requirements, you'll want to bring that up with our hardware department when they design the VIBS keypad. Ken -----Original Message----- From: owner-bugtrack@dieboldes.com [mailto:owner-bugtrack@dieboldes.com]On Behalf Of Larry Dix Sent: Tuesday, September 25, 2001 8:43 AM To: Bugtrack@Gesn. Com Cc: Barry Herron Subject: Numeric Key row inoperable using BS 4.1.1.1 The numeric key row above the qwerty keys is inoperable when plugging in a keyboard for use as an input device for VIBS. The numeric keypad to the right of the keyboard is operable. This creates a problem when demonstrating ADA capabilities using a big key keyboard. The big key keyboard does not have a numeric keypad and therefore can not enter numeric commands. The big key keyboard was selected to meet ADA requirements in Texas that require all controls and operable mechanisms to be operable with one hand including a closed fist. Larry J. Dix Vice President of Operations Global Election Systems

- Follow-Ups:
  - RE: Numeric Key row inoperable using BS 4.1.1.1
    - From: "Ken Clark" <ken@dieboldes.com>

- Prev by Date: RE: BS 4.1.2 Failed to Write to Printer
- Next by Date: RE: BS 4.1.2 Failed to Write to Printer
- Index(es):
  - Chronological
  - Thread