[Date Prev][Date Next] [Chronological] [Thread] [Top]

# FW: Port Server II setup

- To: <support@gesn.com>
- Subject: FW: Port Server II setup
- From: "Ken Clark" <ken@gesn.com>
- Date: Mon, 7 Feb 2000 10:35:20 -0600
- Importance: Normal

Re-posting by popular demand. Who in support is responsible for maintaining this information, or is SOP to call the developers each time we get a new CC account? Ken -----Original Message----- From: Ken Clark [mailto:ken@gesn.com] Sent: Tuesday, July 06, 1999 9:48 AM To: support@gesn.com Subject: RE: Port Server II setup Jeff Hallmark points out there is a missing parameter to the "set user" command: password=off. So, the whole thing becomes: Set config ip=xxx.xxx.xxx.xxx set forwarding state=passive proxyarp=on set ippool count=16 ip=xxx.xxx.xxx.xxx set user name=accuvote protocol=ppp mtu=1500 ipaddr=ippool pppauth=none defaultaccess=netservice netservice=on compression=vj password=off set line baud=19200 range=1-16 set flow altpin=on range=1-16 Ken

- Prev by Date: Re: Gems 1-15-2 & AccuVote 1.94x (and E-Mail to Bug Track) - Withdrawn candidate problems for Puerto Rico
- Next by Date: Re: Modem Setup in GEMS
- Index(es):
  - Chronological
  - Thread