[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AVTS 4.0.4 - Record/Playback Feature

- To: <support@gesn.com>
- Subject: RE: AVTS 4.0.4 - Record/Playback Feature
- From: "Jeff Hintz" <jhglobal@earthlink.net>
- Date: Tue, 10 Jul 2001 13:11:16 -0500
- Importance: Normal
- In-reply-to: <PPECJKNKLDJLKJPKPPIOIEIMCPAA.ken@gesn.com>

The current script set of 8 ballots was set up during the I-Mark days for Wyle testing. Using the 8 ballot script would give us the 300,000 plus votes that we need for the 163 hour continuous test. I would have to rework the numbers & timing for a 6 ballot script.
Larry & Don, is this what we want to do???

> -----Original Message-----
> From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark
> Sent: Tuesday, July 10, 2001 11:29 AM
> To: support@gesn.com
> Subject: RE: AVTS 4.0.4 - Record/Playback Feature
> My educated guess is that it is a fixed buffer. It will work right up to 6, any repeat. Would that be sufficient for now?
> Ken

> > -----Original Message-----
> > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz
> > Sent: Tuesday, July 10, 2001 8:02 AM
> > To: support@gesn.com
> > Subject: RE: AVTS 4.0.4 - Record/Playback Feature
> > I did a 1 ballot test with a repeat of 16. This works fine. I will keep continuing to increase the number of ballots until I can get it to break again.

> > > -----Original Message-----
> > > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark
> > > Sent: Monday, July 09, 2001 4:14 PM
> > > To: support@gesn.com
> > > Subject: RE: AVTS 4.0.4 - Record/Playback Feature
> > > *Exactly* the same result, or does it fail at different points? If you limit your test to say 6 or 7 ballots, does it then work okay?
> > > Ken

> > > > -----Original Message-----
> > > > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz
> > > > Sent: Monday, July 09, 2001 1:58 PM
> > > > To: support@gesn.com
> > > > Subject: RE: AVTS 4.0.4 - Record/Playback Feature
> > > > I have tried it 4 times, all with the same result.
> > > > As soon as I get my laptop to be able to recognize the PCMCIA card, I will send it to you.
> > > > Thanks

> > > > > -----Original Message-----
> > > > > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark
> > > > > Sent: Monday, July 09, 2001 3:22 PM
> > > > > To: support@gesn.com
> > > > > Subject: RE: AVTS 4.0.4 - Record/Playback Feature
> > > > > Repeat it, then send me both scripts if it doesn't work the second try.
> > > > > Ken

> > > > > > -----Original Message-----
> > > > > > From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz
> > > > > > Sent: Monday, July 09, 2001 1:21 PM
> > > > > > To: Support Team (E-mail)
> > > > > > Subject: AVTS 4.0.4 - Record/Playback Feature
> > > > > > I have created a script for voting 8 different ballots, each ballot contains 5 pages, and I have set it up to repeat 64 times. However, when the script gets to the 7th ballot, it skips voting on the the 3rd page, and then when it gets to the final Summary Page it just stays there until you press the F3 key to stop the script.
> > > > > > After I recorded the script, I printed out a report to make sure that I had voted every ballot correctly, and the report was correct.
> > > > > > Any suggestions??? This is the script that we will need to run for the Wyle volume test.
> > > > > > Thanks,
> > > > > > JEFF HINTZ
> > > > > > Global Election Systems

- Follow-Ups:
  - RE: AVTS 4.0.4 - Record/Playback Feature
    - From: "Larry Dix" <ljdglobal@gesn.com>

- References:
  - RE: AVTS 4.0.4 - Record/Playback Feature
    - From: "Ken Clark" <ken@gesn.com>

- Prev by Date: RE: AVTS 4.0.4 - Record/Playback Feature
- Next by Date: RE: AVTS 4.0.4 - Record/Playback Feature
- Index(es):
  - Chronological
  - Thread