[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AVTS 4.0.4 - Record/Playback Feature

- To: <support@gesn.com>
- Subject: RE: AVTS 4.0.4 - Record/Playback Feature
- From: "Larry Dix" <ljdglobal@gesn.com>
- Date: Tue, 10 Jul 2001 16:00:42 -0500
- Importance: Normal
- In-reply-to: <PPECJKNKLDJLKJPKPPIOGEIPCPAA.ken@gesn.com>

Jeff – What amount of time would it take to modify the scripts from 8 to 6 and still be able to reach the 297,000 FEC votes requirement. Larry J. Dix Vice President of Operations Global Election Systems -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark Sent: Tuesday, July 10, 2001 3:01 PM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature Its a bug looks like. There doesn't look to be any deliberate buffer size limit, which would have been straightforward to bump up. I didn't write the code. I'll bang on it a bit, but I am still pending on the "would that be sufficient for now" question. Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Larry Dix Sent: Tuesday, July 10, 2001 11:39 AM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature Ken - What would it take to change this to allow for an eight ballot script? Larry J. Dix Vice President of Operations Global Election Systems -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz Sent: Tuesday, July 10, 2001 1:11 PM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature The current script set of 8 ballots was set up during the I-Mark days for Wyle testing. Using the 8 ballot script would give us the 300,000 plus votes that we need for the 163 hour continuous test. I would have to rework the numbers & timing for a 6 ballot script. Larry & Don, is this what we want to do??? -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark Sent: Tuesday, July 10, 2001 11:29 AM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature My educated guess is that it is a fixed buffer. It will work right up to 6, any repeat. Would that be sufficient for now? Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz Sent: Tuesday, July 10, 2001 8:02 AM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature I did a 1 ballot test with a repeat of 16. This works fine. I will keep continuing to increase the number of ballots until I can get it to break again. -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark Sent: Monday, July 09, 2001 4:14 PM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature *Exactly* the same result, or does it fail at different points? If you limit your test to say 6 or 7 ballots, does it then work okay? Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz Sent: Monday, July 09, 2001 1:58 PM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature I have tried it 4 times, all with the same result. As soon as I get my laptop to be able to recognize the PCMCIA card, I will send it to you. Thanks -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ken Clark Sent: Monday, July 09, 2001 3:22 PM To: support@gesn.com Subject: RE: AVTS 4.0.4 - Record/Playback Feature Repeat it, then send me both scripts if it doesn't work the second try. Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Jeff Hintz Sent: Monday, July 09, 2001 1:21 PM To: Support Team (E-mail) Subject: AVTS 4.0.4 - Record/Playback Feature I have created a script for voting 8 different ballots, each ballot contains 5 pages, and I have set it up to repeat 64 times. However, when the script gets to the 7th ballot, it skips voting on the the 3rd page, and then when it gets to the final Summary Page it just stays there until you press the F3 key to stop the script. After I recorded the script, I printed out a report to make sure that I had voted every ballot correctly, and the report was correct. Any suggestions??? This is the script that we will need to run for the Wyle volume test. Thanks, JEFF HINTZ Global Election Systems

- Follow-Ups:
  - RE: AVTS 4.0.4 - Record/Playback Feature
    - From: "Jeff Hintz" <jhglobal@earthlink.net>

- References:
  - RE: AVTS 4.0.4 - Record/Playback Feature
    - From: "Ken Clark" <ken@gesn.com>

- Prev by Date: RE: AVTS 4.0.4 - Record/Playback Feature
- Next by Date: RE: AVTS 4.0.4 - Record/Playback Feature
- Index(es):
  - Chronological
  - Thread