[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: Central Count Scanner

- To: <support@dieboldes.com>
- Subject: RE: Central Count Scanner
- From: "Jason Wong" <jasonw@dieboldes.com>
- Date: Thu, 25 Jul 2002 12:37:05 -0700
- Importance: Normal
- In-reply-to: <NGBBJFAJENGBILFIMBGFAENACDAA.skglobal@earthlink.net>

    For Central Count, you shouldn't HAVE to run a separate computer to
    connect to the GEMS Central Count server, BUT you may run a separate one
    if you wish.

    Central count has two possibilities for connecting.  One is through PPP
    using the Digi PortServer.  The second is through a RAS connection.  For
    a RAS connection, any computer with an available COM port and connected
    to the network can be used.  This includes the computer running the GEMS
    Central Count Server.

    As far as I am aware however, current released versions of Central Count
    however are not able to connect through RAS on a Windows 2000
    environment but should connect in a Windows NT environment.

    Jason Wong

    -----Original Message-----
    From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf
    Of Steve Knecht
    Sent: July 25, 2002 11:49 AM
    To: Global Support
    Subject: Central Count Scanner

    Do we need to configure a seperate NT/2000 CPU/Server (please specify)
    to
    run central count (scanner option) in addition to the GEMS CPU or can we
    run
    the scanners on GEMS Server?

- Follow-Ups:
  - RE: Central Count Scanner
    - From: "Ken Clark" <ken@dieboldes.com>

- References:
  - Central Count Scanner
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Central Count Scanner
- Next by Date: RE: Permanent Absentee Voters
- Index(es):
  - Chronological
  - Thread