[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Thick vertical lines (Minnesota)

- To: "Support Team (E-mail)" <support@gesn.com>
- Subject: Thick vertical lines (Minnesota)
- From: "Ian Piper" <ian@gesn.com>
- Date: Fri, 14 Apr 2000 16:21:47 -0500

Just a warning to all: If you use thick vertical lines on ballot layout and leave the voting oval in the adjacent column, you will compromise the accuracy of the scanning. Ballot shift in the reader's paper path will cause false marks to be detected in those voting ovals causing a high number of overvoted races. Ensure that the vertical line has one voting column of clearance away from any voting ovals. Ian

- Follow-Ups:
  - Re: Thick vertical lines (Minnesota)
    - From: "Steve Knecht" <skglobal@earthlink.net>

- Prev by Date: Re: 1.16 color features
- Next by Date: AVTS 3.12.5 HAND BITMAP
- Index(es):
  - Chronological
  - Thread