[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AVTS - Fast Card

- To: "Bugs List (E-mail)" <bugtrack@dieboldes.com>
- Subject: RE: AVTS - Fast Card
- From: "Ken Clark" <ken@dieboldes.com>
- Date: Tue, 7 Sep 1999 16:36:28 +0100
- Importance: Normal
- In-Reply-To: <01BEF918.ED344670@sdn-ar-003neomahP254.dialsprint.net>

    What is the bug?  I am not sure what "no writing" and "has writing" means,
    but this all sounds about right.  You only get 3 seconds using CLXSA001, as
    explained on the rcr list.  I guess that means your "has writing card" --
    but I wouldn't know.  The 3 second card I tested with is square but I can't
    see any writing on it.  I haven't tried the "L Shaped" type.

    Other cards behave the same as before (maybe a fraction worse), although
    around 16-20 seconds is now split between the opening screen and the record
    results screen -- effectively cutting in half the opening screen time worst
    case.

    Ken
    PS are you going to fix your mailer to do HTML or not?

    > -----Original Message-----
    > From: owner-bugtrack@dieboldes.com [mailto:owner-bugtrack@dieboldes.com]On Behalf
    > Of Jeff Hintz
    > Sent: Tuesday, September 07, 1999 4:08 PM
    > To: Bugs List (E-mail)
    > Subject: AVTS - Fast Card
    >
    >
    > I have just finished testing the new fast card reading software.
    > Using the old oval shaped Smart Card & the square shaped Smart
    > Card with no writing, it takes about 10 seconds to read the card
    > and then about 10 seconds to write to the card after you hit Cast
    > Ballot.  The square shaped Smart Card that has writing that says
    > ATMEL on it, takes about 3 seconds to read the card and then
    > about 10 seconds to write to the card after you hit Cast Ballot.
    >
    > Jeff Hintz
    > Global Election Systems
    >

- References:
  - AVTS - Fast Card
    - From: Jeff Hintz <jhglobal@earthlink.net>

- Prev by Date: AVTS - Fast Card
- Next by Date: RE: Gaston
- Index(es):
  - Chronological
  - Thread