[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: What works with what?

- To: <support@gesn.com>
- Subject: RE: What works with what?
- From: "Ken Clark" <ken@gesn.com>
- Date: Tue, 11 Jun 2002 09:25:40 -0800
- Importance: Normal
- In-reply-to: <010801c21163$17957320$0203a8c0@desktop>

Hmm, it won’t be on your laptop – dlls on the AVTS are not compatible with those on your laptop. Fmodce.dll should have been installed automatically when you upgraded to 4.3.x. If you are running 4.3.x on your laptop under NT (not R6 Ballot Station as you said) then you might have a problem. Dmitry can supply you with the NT dll for fmod. Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf Of Steve Knecht Sent: Tuesday, June 11, 2002 8:15 AM To: support@gesn.com Subject: Re: What works with what? I'm getting there thanks. Running into a new message about missing fmod.dll, but I'm sure it must be on my laptop somewhere. ----- Original Message ----- From: Ken Clark To: support@gesn.com Sent: Monday, June 10, 2002 6:06 PM Subject: RE: What works with what? It would help if you could have elaborated on “older ballot station versions”, but yes, your PCMCIA card is not compatible with the ballot station you are using. It would probably be nice if the error message were a little friendlier than just “bad DLD”, which is a pretty meaningless error. The problem isn’t really with MP3 vs PCM, as you can indeed mix and match with ballot station 4.3.x. The problem is that you are trying to put a 4.[012].x memory card into a 4.3 machine. Ken -----Original Message----- From: owner-support@gesn.com [mailto:owner-support@gesn.com] On Behalf Of Steve Knecht Sent: Monday, June 10, 2002 3:46 PM To: Global Support Subject: What works with what? I've got an R6 ballot station with 4.3.7 and CE 3.0 loaded. My older Alameda PCMCIA that works with older ballot station versions give me a "bad DLD" file error when I insert it. If I create a new ballot station with GEMS 1.18.10 and the new MP3 instruction audio, and redownload a PCMCIA, will the old audio work for the races and candidates? I guess the question could also be stated "can we combine PCM and MP3 formats"?

- References:
  - Re: What works with what?
    - From: "Steve Knecht" <stevek@gesn.com>

- Prev by Date: Re: changing BS format
- Next by Date: RE: changing BS format
- Index(es):
  - Chronological
  - Thread