[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: GEMS-1-14-11, GEMS-1-15-5

- To: "Dmitry Papushin" <dmitry@gesn.com>, <support@gesn.com>
- Subject: Re: GEMS-1-14-11, GEMS-1-15-5
- From: "Steve Knecht" <skglobal@earthlink.net>
- Date: Tue, 22 Feb 2000 16:06:58 -0800

Please send the GEMS version WITH the version numbers like this: GEMS-1-14-11.exe This way people won't have to rename their GEMS file all the time, potentially getting confused on their versions. They can run their GEMS 1-14-11 from an icon that specifies their version number just as easily as doing it with the GEMS only name. -----Original Message----- From: Dmitry Papushin <dmitry@gesn.com> To: Software Announcements <sw-announce@gesn.com> Date: Tuesday, February 22, 2000 1:54 PM Subject: GEMS-1-14-11, GEMS-1-15-5 GEMS-1-14-11 and GEMS-1-15-5 are ready. The passwords are: GEMS-1-15-5.zip ckt4hfhsvedsv GEMS-1-14-11.zip deg4t5klkfbsf 1.15.5 · Improve 1.9x modem handling. · Turn local echo off so we don't mistake echos for an AV. · Detect that we are attached to an modem even if we are online. · Close and reopen the port if we get an IO exception. · Detect loss of carier during RTS exchange. · Improve user feedback of status · Implement server connect timeout · Don't include label candidates in upload candidate maps · Fix bug which caused print artwork to fail 1.14.11 · Improve 1.9x modem handling. · Turn local echo off so we don't mistake echos for an AV. · Detect that we are attached to an modem even if we are online. · Close and reopen the port if we get an IO exception. · Detect loss of carier during RTS exchange. · Improve user feedback of status Dmitry

- Prev by Date: Re: GEMS-1-14-11 Modem Handling
- Next by Date: RE: GEMS-1-14-11 Modem Handling
- Index(es):
  - Chronological
  - Thread