[Date Prev][Date Next] [Chronological] [Thread] [Top]

# Re: R6 modem testing successful

- To: <support@gesn.com>
- Subject: Re: R6 modem testing successful
- From: ian@gesn.com
- Date: Sat, 26 Jan 2002 09:58:46 -0600 (CST)
- Cc: <tiredale@gesn.com>
- Importance: Normal
- In-reply-to: <023c01c1a606$a07cc2b0$1404a8c0@gesn.com>
- References: <023c01c1a606$a07cc2b0$1404a8c0@gesn.com>

    Tab:

    What versions of Windows CE and Ballot Station Software did you perform
    this testing?

    Ian

    I have tested the following modems, sent to me by Ian, with AccuVote-TS
    > R6 unit.
    >
    > The following modems successfully uploaded to GEMS:
    >    ActionTec DataLik 33.6 kbps V.34+ Fax/Modem
    >    Zoom V.92 Pc Card Modem
    >    MultiTec MultiMobile 56K Modem
    >    PC_Card v.90 Modem
    >
    > The Hawkings 56K V.90 Fax/Modem locked up the system while it was
    > inserted.  I will try to determine the cause for this but in the mean
    > time do not use this type of modem.
    >
    > Tab
    >
    >
    >  ----- Original Message -----
    >  From: Tari Runyan
    >  To: Support
    >  Sent: Wednesday, January 16, 2002 2:46 PM
    >  Subject: R6 modem testing successful
    >
    >
    >  I purchased a ThinFax 56L low power 56K PCMCIA modem for the R6 for
    >  60.09 and tested it successfully - thanks to Jeff Hintz's tips -  it
    >  is plug and play - all you do is enter the phone number and IP address
    >  - or host name and it uploads  I got it from www.Provantage.com
    >
    >  Tari Runyan

- Follow-Ups:
  - Re: R6 modem testing successful
    - From: "Steve Knecht" <skglobal@earthlink.net>
  - Re: R6 modem testing successful
    - From: "Talbot Iredale" <tiredale@gesn.com>

- References:
  - Re: R6 modem testing successful
    - From: "Talbot Iredale" <tiredale@gesn.com>

- Prev by Date: Re: How to restore if PCMCIA goes south
- Next by Date: Re: R6 modem testing successful
- Index(es):
  - Chronological
  - Thread