[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AVOS/TS blended system uploads

- To: <support@dieboldes.com>
- Subject: RE: AVOS/TS blended system uploads
- From: "Cathi Smothers" <cathis@dieboldes.com>
- Date: Fri, 24 Jan 2003 10:49:41 -0500
- Importance: Normal
- In-reply-to: <APEKLJFKJOPPBMGOIEONKELGCFAA.marke@dieboldes.com>

Mark, With the Polling Vote Center expanded in the tree view, click on Pct 1 OS. Then hold down the shift and control keys and drag and drop the Pct 1 report precinct from the right side over to Pct 1 TS. This should allow you to duplicate the report precinct within the Polling vote center category. Cathi -----Original Message----- From: owner-support@dieboldes.com [mailto:owner-support@dieboldes.com]On Behalf Of Mark Earley Sent: Friday, January 24, 2003 10:26 AM To: support@dieboldes.com Subject: RE: AVOS/TS blended system uploads Nel, I cannot get a report precinct to attach to more than one vote center within the Polling vote center group. It does work if I make a separate counter group called Polling TS vote centers. See attached db. This is an old db so the password is "global". I configured the two Polling Vote Centers (OS and TS) without the cumulative results only check box checked. Am I doing something wrong? Mark -----Original Message----- From: owner-support@dieboldes.com [mailto:owner-support@dieboldes.com]On Behalf Of Nel Finberg Sent: Thursday, January 23, 2003 8:11 PM To: support@dieboldes.com Subject: RE: AVOS/TS blended system uploads Mark, you don't need a unique vote center category to configure the blended system, just define two vote centers for every polling location, all in the same vote center category (assuming both AccuVote-OS and AccuVote-TS units are used for polling). Nel -----Original Message----- From: owner-support@dieboldes.com [mailto:owner-support@dieboldes.com] On Behalf Of Mark Earley Sent: January 23, 2003 4:31 PM To: Support Subject: AVOS/TS blended system uploads With the new ADA requirements facing our OS customers, they will likely be knocking on our door to purchase TS units to compliment their existing OS systems with one TS unit in each precinct - coexisting with the OS units in a blended system. While there are some problems with programming such a system (namely needing to have another Vote Center category created for the TS units), these are hurdles that can be managed (I guess they can - does anyone have thoughts on this?). My bigger concern is handling the uploading of both TS and OS results via modem into the GEMS server. What are the known issues relating to upload? I know that TS uses RAS while OS uses regular serial com ports, thus the need for separate modem banks. Can GEMS receive modem uploads from both OS and TS units at the same time? Has this been tested in any kind of a medium to large scale test? Does anyone have any experience with receiving both TS and OS modem uploads? Thanks. Mark Mark Earley 850 422-2100 - office/fax 850 322-3226 – cell

- Follow-Ups:
  - RE: AVOS/TS blended system uploads
    - From: "Mark Earley" <marke@dieboldes.com>

- References:
  - RE: AVOS/TS blended system uploads
    - From: "Mark Earley" <marke@dieboldes.com>

- Prev by Date: RE: GEMS-1-18-17
- Next by Date: RE: AVOS/TS blended system uploads
- Index(es):
  - Chronological
  - Thread