[Date Prev][Date Next] [Chronological] [Thread] [Top]

# RE: AVOS-PC-FC-194x

- To: <support@gesn.com>
- Subject: RE: AVOS-PC-FC-194x
- From: "Ken Clark" <ken@gesn.com>
- Date: Mon, 17 Sep 2001 16:27:41 -0700
- Importance: Normal
- In-reply-to: <019201c13fca$9c8f8680$3c03a8c0@obrien>

Same as always for 1.9[456] releases: both A&B will fit on 64kbyte chips. You can of course burn the same hex files onto larger chips if you like. If they are using the bigger clock chip, you can use 128kbyte chips.
Ken

> -----Original Message-----
> From: owner-support@gesn.com [mailto:owner-support@gesn.com]On Behalf Of Ian S. Piper
> Sent: Monday, September 17, 2001 3:47 PM
> To: support@gesn.com
> Subject: RE: AVOS-PC-FC-194x
> What are the chip sizes for this release?
> Ian

> > -----Original Message-----
> > From: owner-sw-announce@gesn.com [mailto:owner-sw-announce@gesn.com]On Behalf Of Ken Clark
> > Sent: September 17, 2001 5:24 PM
> > To: sw-announce@gesn.com
> > Subject: AVOS-PC-FC-194x
> > AccuVote OS Precinct Count French Canadian 1.94x is ready. Its in the AVOSFix directory. The firmware checksums are A:6A32 B:92E9.
> > AVOS-PC-FC-194x.zip obhrt4iypfndh

- Follow-Ups:
  - RE: AVOS-PC-FC-194x
    - From: "Ian S. Piper" <ian@gesn.com>

- References:
  - RE: AVOS-PC-FC-194x
    - From: "Ian S. Piper" <ian@gesn.com>

- Prev by Date: RE: AVOS-PC-FC-194x
- Next by Date: Keypad
- Index(es):
  - Chronological
  - Thread